COUlthardyne systems

Proudly introduces:

**THE catinatorTM**

The world’s first cybernetic Animal trap

Series: 100

Model: 101

Serial #: 000000000x

General description:

infiltration unit: part plant, part machine. hyperalloy Trapping chassis, microprocessor-controlled. Fully armored; very tough. But outside, living plant tissue: leaves, branches, wood...

facts/features:

* 1.2GHz 64-bit quad-core ARMv8 CPU
* 1GB RAM/64gb hard disk
* 4 USB ports/40 GPIO pins (2 in use)
* Full HDMI port/Ethernet Port
* Combined 3.5mm audio jack and composite video
* webcam with real-time viewing
* GSM/UMTS/HSPA+850/1900/2100 Mhz
* 802.11n Wireless LAN
* Bluetooth 4.1 and Bluetooth Low Energy (BLE)
* Battery ca[pacity: 30000 mAH
* Battery duration: 4 days
* 3 tier notification system:
  + Sms/Plain text email/html email
* Solar recharghing
* Low power mode
* Noip ddns support